|  |
| --- |
| **GAUGE** |
| **Gauge Type:** | [ ]  Reflex | [ ]  Transparent | **Style:** | [ ]  Medium Pressure | [ ]  High Pressure |
| **Connection Size:** | [ ]  ½” | [ ]  ¾” | [ ]  1” | [ ]  1 ½” | [ ]  2” | [ ]  3” | [ ]  4” | [ ]  6” | [ ]  8” |
| **Connection Type** | [ ]  NPT | [ ]  Socketweld | [ ]  Flange Click or tap here to enter text. |
| **Connection Location:** | [ ]  End [ ]  Side (Left) [ ]  Side (Right) [ ]  Back | Additional Conn: | [ ]  Vent [x]  Drain |
| **Vessel C-C Dimension:** | Click or tap here to enter text. inches |
| **Chamber Material:** CS NACE | **Cover Material:** CS NACE |
| **Gasket/Cushion Material:** HPN | **Glass:** BOROSILICATE |
| **Design Rating:** Click or tap here to enter text.°F @ Click or tap here to enter text.psig |
| **Options**: [ ]  Illuminator [ ]  Frost-proof Extension [ ]  Shield [ ]  Gauge Scale [ ]  Internal Heating [ ]  External Heating [ ]  Off Shore Paint [ ]  Thermal Blanket |
| **Other Requirements:** Click or tap here to enter text. |

|  |
| --- |
| **VALVES** |
| [ ]  **Assemble to Gauge** |
|  |
| **Material:**  | **Body:** CS NACE | **Trim:** 316SS | **Packing:** TFE |
| **Vessel Connection Size:** | [ ]  ½” | [ ]  ¾” | [ ]  1” | [ ]  1 ½” | [ ]  2” | [ ]  3” | [ ]  4” | [ ]  6” | [ ]  8” |
| **Vessel Connection Type:** | [ ]  NPT | [ ]  Socketweld | [ ]  Flange  |
| **Vessel Connection Style:** | [ ]  Male Union [ ]  Female Union  |
| **Gauge Connection Size:** | [ ]  ½” [ ]  ¾” |
| **Gauge Connection Type:** | [ ]  NPT | [ ]  Socketweld | [ ]  Flange  |
| **Gauge Connection Style:** | [ ]  Male Union [ ]  Female Union  |
| **Vent/Drain Connect. Size:** | [ ]  ½” [ ]  ¾” [ ]  Other Click or tap here to enter text. |
| **Vent/Drain Connect. Type:** | [ ]  NPT [ ]  Socketweld [ ]  Other Click or tap here to enter text. |
| **Bonnet:** | [ ]  Integral [ ]  Union |
| **Quick Closing:** | [ ]  Lever [ ]  Handwheel |
| **Other Requirements:** |
| Click or tap here to enter text. |